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	No
	Name of Projects and Brief Description
	Role
	Employer
	Remark

	1
	Geotechnical Investigation Services for Five River Bridges under Serofta – Warqa Design Project
	Sole Consultant
	VALUE Engineering PLC
	Completed

	2
	Geotechnical Investigation for Three Span Mena River for Amhara Rural Roads Authority
	Sole Consultant
	NOMY Engineering PLC
	Completed

	3
	Geotechnical Investigation for Two Boreholes to 20m depth for 2B+G+8 MIXED USE BUILDING (Addis Ababa, CMC Summit Area)
	Sole Consultant
	NOMY Engineering PLC
	Completed

	4
	Geotechnical Investigation for Two Boreholes to 15m depth for B+G+4 MIXED USE BUILDING (Addis Ababa, CMC Summit Area
	Sole Consultant
	NOMY Engineering PLC
	Completed

	5
	Geotechnical Investigation of Four Boreholes in Gambella Regional State Water Well Drilling & Supply Project
	Sole Consultant
	Zekalay General Trading PLC
.
	Completed

	6
	Foundation Investigation for the construction of Administrative building & staff accommodations (4 Bore holes)
	Sole Consultant
	BNT Industry & Trading PLC
	Completed







	Assignment Name:
Geotechnical Investigation Services for Five River Bridges under Serofta – Warqa Design Project
	Approx. value of the contract 
 ETB 3,500,000.00

	 Country:
 Ethiopia

 Location within Country:
West Region, Ethiopia 
	 Duration of Assignment:2 months
No. of Staff:	6
No. of Staff Months:12 man-months

Professional Staff Provided by the Firm:
· Senior Geotechnical Engineer
· Geotechnical Engineer
· Chief Driller
· Assistant Drillers
· Labourers

	 Name of Client: VALUE Engineering PLC Employer: Ethiopian Roads Authority
	

	Address: Ethiopian Roads Authority
P.O.Box 1770, Tel.: 251-115- 156603
	

	Legal /Contractual status of the firm
(sole consultant, joint venture, sub-consultant)

	Start Date:
June 2012
	Completion Date:
August 2012
	Approx. Value of Services:
ETB 1, 300,000.00

	Name of Associated Firm(s) if any: 
None
	No. of Months of Professional Staff provided by Associated Firm(s): -

	Name of Senior Staff (Project Director/ Co-ordinator, Team Leader) involved and functions performed: 
· Demelash Samuel, Senior Geotechnical Engineer (Team Leader)
· Henock Tesfaye (Geologist)

	Narrative Description of Project:
· Geotechnical Investigation Services, bearing capacity determination & foundation recommendation.

	Description of Actual Services Provided by ECSE staff:

· Carry out Geological Investigation on the proposed bridge alignment of the road
· Develop a full site investigation program.
· Mobilization & demobilization of 2drilling rigs with all facilities, accessories, equipment and crew.
· Enter bore hole and enter site movement. 
· Undertake & carryout filled exploration by using rotary core drilling for 10 boreholes to 20m depth
· Sampling & Testing including SPT test, undisturbed soil sampling, disturbed soil sampling, rock core sampling, ground water level measurement, ground water sampling & logging of bore holes including provision of core box & photographing. 
· Carryout central laboratory testing including natural moisture content, density, specific gravity, grain size analysis, atterberg limits, undrained tri-axial tests, unconfined compressive strength, consolidated tests, direct shear box test, dry density, specific gravity, comprehensive strength & water absorption on rock cores, soluble sulphate& chloride content in soil & water & unit wait determination. 
· Conduct Geotechnical & stability analysis
· Provide Design recommendation based on the results of the foundation investigation
· Prepare Geotechnical Engineering Report showing layout plan, description of sub-soil condition & sub-surface strata, results of field & Laboratory test, observation & analysis, estimate of allowable loading and bearing capacity, settlement consideration, corrosion effect of soil & water encountered, recommendation on type & depth of foundation and bore hole logs & photographs. 


Current status: 		The Service is 100% Completed.


	Assignment Name:
Geotechnical Investigation for Three Span Mena River for Amhara Rural Roads Authority
	Approx. value of the contract 
N/A

	 Country:
Gonder, Ethiopia
 Location within Country: Amhara Regional State

	 Duration of Assignment:3 month
No. of Staff:	5
No. of Staff Months:15

Professional Staff Provided by the Firm: 
· Senior Geotechnical Engineer
· Geologist
· Chief Drilling Technician
· Assistant Drillers
· Labourers

	 Name of Client: NOMY Engineering PLC
	

	Address: NOMY Engineering PLC
Tel.: 251-11- 646 04 08, Fax.: 251-11-646 03 76
Addis Ababa, Ethiopia
	

	Legal /Contractual status of the firm
(sole consultant, joint venture, sub-consultant)

	Start Date:

November 2014
	Completion Date:

December 2015
	Approx. Value of Services  :
ETB 220,000.00

	Name of Associated Firm(s) if any: 
None
	No. of Months of Professional Staff provided by Associated Firm(s): -

	Name of Senior Staff (Project Director/ Co-ordinator, Team Leader) involved and functions performed: 
· Demelash Samuel, Senior Geotechnical Engineer (Team Leader)
· Henock Tesfaye (Geologist)
· Assefa Ababu(Chief Drilling Technician)

	Narrative Description of Project:
· Geotechnical Investigation of Mena River Bridges Project

	Description of Actual Services Provided by ECSE staff:
· Carry out Geological Investigation on the proposed bridge alignment of the road
· Develop a full site investigation program.
· Undertake & carryout field exploration by using rotary core drilling for 10 boreholes to 20m depth
· Sampling & Testing including SPT test, undisturbed soil sampling, disturbed soil sampling, rock core sampling, ground water level measurement, ground water sampling & logging of bore holes including provision of core box & photographing.
· Carryout central laboratory testing including natural moisture content, density, specific gravity, grain size analysis, atterberg limits, undrained tri-axial tests, unconfined compressive strength, consolidated tests, direct shear box test, dry density, specific gravity, comprehensive strength & water absorption on rock cores, soluble sulphate& chloride content in soil & water & unit wait determination. 
· Conduct Geotechnical & stability analysis
· Provide Design recommendation based on the results of the foundation investigation
· Prepare Geotechnical Engineering Report showing layout plan, description of sub-soil condition & sub-surface strata, results of field & Laboratory test, observation & analysis, estimate of allowable loading and bearing capacity, settlement consideration, corrosion effect of soil & water encountered, recommendation on type & depth of foundation and bore hole logs & photographs.


Current status: 		The Service is 100% Completed.

	Assignment Name:
Geotechnical Investigation for Two Boreholes to 20m depth for 2B+G+8 MIXED USE BUILDING (Addis Ababa, CMC Summit Area)
	Approx. value of the contract 
N/A

	 Country:
 Ethiopia
 Location within Country:Addis Ababa

	 Duration of Assignment:0.25 month
No. of Staff:	 6
No. of Staff Months:

Professional Staff Provided by the Firm: 
· Senior Geotechnical Engineer
· Geotechnical Engineer
· Chief Drilling Technician
· Assistant Drillers
· Labourers

	 Name of Client:NOMY Engineering PLC
	

	Address:NOMY Engineering PLC
Tel.: 251-11- 646 04 08, Fax.: 251-11-646 03 76
Addis Ababa, Ethiopia 
	

	Legal /Contractual status of the firm
(sole consultant, joint venture, sub-consultant)

	Start Date:

December 2014
	Completion Date:

January 2015
	Approx. Value of Services  :
ETB 51,000.00

	Name of Associated Firm(s) if any: 
None
	No. of Months of Professional Staff provided by Associated Firm(s): -

	Name of Senior Staff (Project Director/ Co-ordinator, Team Leader) involved and functions performed: 
· Demelash Samuel, Senior Geotechnical Engineer (Team Leader)
· Henock Tesfaye (Geologist)
· Mekitachew Teshome(Chief Drilling Technician)


	Narrative Description of Project:
· Geotechnical Investigation of Two Boreholes to 20m depth for 2B+G+8 MIXED USEBUILDING


	Description of Actual Services Provided by ECSE staff:
· Mobilization of 1 drilling rig along with accessories and crew, Deep vertical rotary core drilling at 2 boreholes upto a depth of 20m, field tests (SPT, CPT, undisturbed soil sampling, disturbed soil sampling, ground water measurement), different laboratory tests and geotechnical analysis including determination of bearing capacity and recommendation of foundation types and depth.



Current status: 		The Service is 100% Completed.





	Assignment Name:
Geotechnical Investigation for Two Boreholes to 15m depth for B+G+4 MIXED USE BUILDING (Addis Ababa, CMC Summit Area)
	Approx. value of the contract 
N/A

	 Country:
 Ethiopia
 Location within Country:Addis Ababa

	 Duration of Assignment:0.25 month
No. of Staff:	 6
No. of Staff Months:

Professional Staff Provided by the Firm: 
· Senior Geotechnical Engineer
· Geotechnical Engineer
· Chief Drilling Technician
· Assistant Drillers
· Labourers

	 Name of Client:NOMY Engineering PLC
	

	Address:NOMY Engineering PLC
Tel.: 251-11- 646 04 08, Fax.: 251-11-646 03 76
Addis Ababa, Ethiopia 
	

	Legal /Contractual status of the firm
(sole consultant, joint venture, sub-consultant)

	Start Date:

December 2014
	Completion Date:

January 2015
	Approx. Value of Services  :
ETB 51,000.00

	Name of Associated Firm(s) if any: 
None
	No. of Months of Professional Staff provided by Associated Firm(s): -

	Name of Senior Staff (Project Director/ Co-ordinator, Team Leader) involved and functions performed: 
· Demelash Samuel, Senior Geotechnical Engineer (Team Leader)
· Henock Tesfaye (Geologist)
· Mekitachew Teshome(Chief Drilling Technician)


	Narrative Description of Project:
· Geotechnical Investigation of Two Boreholes to 15m depth for B+G+4 MIXED USEBUILDING


	Description of Actual Services Provided by ECSE staff:
· Mobilization of 1 drilling rig along with accessories and crew, Deep vertical rotary core drilling at 2 boreholes upto a depth of 15m, field tests (SPT, CPT, undisturbed soil sampling, disturbed soil sampling, ground water measurement), different laboratory tests and geotechnical analysis including determination of bearing capacity and recommendation of foundation types and depth.



Current status: 		The Investigation Work is Complete




	Assignment Name:
Geotechnical Investigation of Four BoreholesinGambella Regional State Water Well Drilling & Supply Project
	Approx. value of the contract 
N/A

	 Country:
 Ethiopia
 Location within Country:WestRegion
	 Duration of Assignment: 1 month
No. of Staff:	 6
No. of Staff Months:6
Professional Staff Provided by the Firm: 
· Senior Geotechnical Engineer
· Geotechnical Engineer
· Chief Drilling Technician
· Assistant Drillers
· Labourers

	 Name of Client:Zekalay General Trading PLC

	

	Address:Zekalay General Trading PLC
Tel.: 251-116-45-27-27, Fax. 251-116-466945
E-mail: zekalay@ethionet.et
Addis Ababa, Ethiopia
	

	Legal /Contractual status of the firm
(sole consultant, joint venture, sub-consultant)

	Start Date:
21st August 2014
	Completion Date:
23rd September 2014
	Approx. Value of Services:
ETB 320,000.00

	Name of Associated Firm(s) if any:
None
	No. of Months of Professional Staff provided by Associated Firm(s): -

	Name of Senior Staff (Project Director/ Co-ordinator, Team Leader) involved and functions performed:

· Demelash Samuel, Senior Geotechnical Engineer (Team Leader)
· HenockTesfaye (Geologist)
· MekitachewTeshome(Chief Drilling Technician)


	Narrative Description of Project:
· Geotechnical Investigation of four boreholesto a depth of 30m.

	Description of Actual Services Provided by ECSE staff:
· Mobilization of 1 drilling rig along with accessories and crew, deep vertical rotary core drilling at 4 boreholes up to a depth of 30m, field tests (SPT, CPT, undisturbed soil sampling, disturbed soil sampling, ground water measurement), different laboratory tests and geotechnical analysis including determination of bearing capacity and recommendation of foundation types and depth.


Current status: 		The Investigation Work is Complete






	Assignment Name:
Geotechnical Investigation of Six Boreholes in Afar Regional State Water Well Drilling & Supply Project
	Approx. value of the contract 
N/A

	 Country:
 Ethiopia
 Location within Country:North-Eastern part
	 Duration of Assignment: 1.5 month
No. of Staff:	 6
No. of Staff Months: 9.0
Professional Staff Provided by the Firm: 
· Senior Geotechnical Engineer
· Geotechnical Engineer
· Chief Drilling Technician
· Assistant Drillers
· Labourers

	 Name of Client:Zekalay General Trading PLC

	

	Address:Zekalay General Trading PLC
Tel.: 251-116-45-27-27, Fax. 251-116-466945
E-mail: zekalay@ethionet.et
Addis Ababa, Ethiopia
	

	Legal /Contractual status of the firm
(sole consultant, joint venture, sub-consultant)

	Start Date:
1st October 2014
	Completion Date:
23rd November 2014
	Approx. Value of Services:
ETB 420,000.00

	Name of Associated Firm(s) if any:
None
	No. of Months of Professional Staff provided by Associated Firm(s): -

	Name of Senior Staff (Project Director/ Co-ordinator, Team Leader) involved and functions performed:

· Demelash Samuel, Senior Geotechnical Engineer (Team Leader)
· HenockTesfaye (Geologist)
· MekitachewTeshome(Chief Drilling Technician)


	Narrative Description of Project:
· Geotechnical Investigation of six boreholesto a depth of 30m.

	Description of Actual Services Provided by ECSE staff:
· Mobilization of 1 drilling rig along with accessories and crew, deep vertical rotary core drilling at 6 boreholes up to a depth of 30m, field tests (SPT, CPT, undisturbed soil sampling, disturbed soil sampling, ground water measurement), different laboratory tests and geotechnical analysis including determination of bearing capacity and recommendation of foundation types and depth.


Current status: 		The Investigation Work is Complete









	Assignment Name:
Foundation Investigation for the construction of Administrative building & staff accommodations (4 Bore holes) 
	Approx. value of the contract 
N/A

	 Country:
 Ethiopia
 Location within Country:North-Eastern part
	 Duration of Assignment: 2 weeks 
No. of Staff:	 6
No. of Staff Months: 9.0
Professional Staff Provided by the Firm: 
· Senior Geotechnical Engineer
· Geotechnical Engineer
· Chief Drilling Technician
· Assistant Drillers
· Labourers

	 Name of Client:BNT Industry & Trading PLC

	

	Address: BNT Industry & Trading PLC
Tel.: 251911214063/4893, Fax. 251-115580002
E-mail: bnt.coffee@Yahoo.com, Bire@bntcoffee.com, 
Addis Ababa, Ethiopia
	

	Legal /Contractual status of the firm
(sole consultant, joint venture, sub-consultant)

	Start Date:
1st October 2018
	Completion Date:
16th  October 2018
	Approx. Value of Services:


	Name of Associated Firm(s) if any:
None
	No. of Months of Professional Staff provided by Associated Firm(s): -

	Name of Senior Staff (Project Director/ Co-ordinator, Team Leader) involved and functions performed:

· Demelash Samuel, Senior Geotechnical Engineer (Team Leader)
· HenockTesfaye (Geologist)
· MekitachewTeshome(Chief Drilling Technician)


	Narrative Description of Project:
· Geotechnical Investigation of six boreholesto a depth of 30m.

	Description of Actual Services Provided by ECSE staff:
· Mobilization of 1 drilling rig along with accessories and crew, deep vertical rotary core drilling at 6 boreholes up to a depth of 30m, field tests (SPT, undisturbed soil sampling, disturbed soil sampling, ground water measurement), different laboratory tests and geotechnical analysis including determination of bearing capacity and recommendation of foundation types and depth.


Current status: 		The Investigation Work is Complete
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